WTC

1. **"Sending packet\r\n"**
2. See PI
3. *If “OK “ continue, else* ***"ERR..EOT\r\n"***
4. **"|-----------32-BYTES-----------|”**
5. See PI
6. *If “OK “ continue, else resend (attempt 6 times)*

*If attempt is over 6 times* ***"ERR..EOT\r\n"***

1. **"|-----------32-BYTES-----------|”**
2. See PI
3. *If “OK “ continue, else resend (attempt 6 times)*

*If attempt is over 6 times "ERR..EOT\r\n"*

1. **"|-----------32-BYTES-----------|”**
2. See PI
3. *If “OK “ continue, else resend (attempt 6 times)*

*If attempt is over 6* ***times "ERR..EOT\r\n"***

1. **"|-----------32-BYTES-----------|”**
2. See PI
3. *If “OK “ continue, else resend (attempt 6 times)*

*If attempt is over 6 times "ERR..EOT\r\n"*

1. **"send back\r\n"**
2. See PI
3. *If memcmp == 0* ***"OK..EOT\r\n"***

*else* ***"ERR..EOT\r\n"***

Pi

1. See WTC
2. **“OK “**
3. See WTC
4. See WTC
5. **“OK “**
6. See WTC
7. See WTC
8. **“OK “**
9. See WTC
10. See WTC
11. **“OK “**
12. See WTC
13. See WTC
14. **“OK “**
15. See WTC

1. See WTC
2. **"|-----------32-BYTES-----------||-----------32-BYTES-----------||-----------32-BYTES-----------||-----------32-BYTES-----------|”**
3. See WTC